To respond to these needs, you will be introduced to the topic door control.

Basis for the opening of the front and rear doors is setting the station brake. The switch is located on the lower right end of the instrument panel and can also be (de-)activated with the [Num -] key. Once the the station brake is engaged (only during standstill), the rear doors open automatically if a passenger had pressed the stop request button. Once the running board at the exit is free, the back doors automatically close again after some time. The front doors are opened and closed manually, of course only after engaging the station brake .

- Insert the station brake

- The rear doors open due to the passenger wishes automatically
- Observe the process with the passenger point of view [F2]
- After some time, the rear doors close automatically
- Opening the doors will turn off the stop request indicator

- Open both front doors with the keys [Num /] and [Num *], begin by using the corresponding view of the doors from the driver's position
- Close both front doors again

For bulky items (buggies , wheelchairs) to enter the bus through the back door, you can block the automatic opening and closing of the back doors and open it manually. Use the switch above the station brake. The indicator light buggy request turns off.

If the entry process is complete, you can remove the rear door locking by clicking the switch back to the front. Please test this process now.

The position of the switch station brake is no reliable information on the status of the station brake! Example: Turn off the switch, the brake is still active as long as the rear doors are not closed. On the other hand, the station brake is released immediately when the electricity is turned off or is broken - even when the switch is still turned on.

If all processes are completed, release the station brake again.