[friendlyname]
MAN
SD200 - SD80 (Ticket Printer)
Beige

[description]
Like its predecessors SD78.2 and SD79, the 70 buses of SD80 stock follow the principles of "passenger flow". Thus, these buses feature a second staircase behind the driver's seat for one-way access to the upper deck. The new design of the side rollsign in two separate chambers above the front door has been adopted from these predecessor series, too. A new feature in the SD80 stock is the rearwards facing seat bench next to the buggy place. Passengers wanting to enter the bus with a buggy can inform the driver by pushing a button next to the rear door.
Fitted with new velours seats, The buses no. 1721-1745 differ from the others which still have the older red synthetic leather seat covers.

- Technical Specifications -

Length: 11.490 mm
Width: 2500 mm
Height: 4060 mm

Engine: MAN D2566MUH, 141 kW at 2100 RPM
Gearbox: Voith D851
Maximum speed: 75 km/h

Empty weight: 10700 kg
Gross weight: 16.000 kg

Seats upper deck: 47
Seats lower deck: 34
Standing places: 8
[end]