Now you can try out features for the first time. You will start the engine now step by step.

- Insert the key
- Press the main switch to turn on the electrics
- Turn on your workplace lighting

Start the engine by pressing the starter until the engine is running. To start the engine, no gear must be engaged - which it is at this moment.

Switch off the motor again by pressing the engine shut down until the engine is off .

Release the parking brake by moving the lever forwardly. The indicator light "parking brake engaged" goes black. The parking brake is applied by spring force and released by compressed air. As a consequence, with too low pressure in the tank, the brake is always guaranteed.

Set the parking brake off again, by pulling the lever towards yourself. The indicator light "parking brake engaged" lights up again.

The engine cooling system is activated automatically as required when the engine is running, and also disabled, but you can turn it on manually using the switch. Please try the corresponding switch on the operation panel.