
[friendlyname]
MAN
SD200 - SD83 Rollsign
Beige

[description]
The buses no. 3272-3321 of SD83 stock are the last SD200 fitted with rollsigns. With this advanced system, destination and line number can be preselected - the rollsigns then move into position fully automatically. There is no need to crank the line number manually and thus, accessibility of the rollsign cases can be neglected. The side rollsigns are therefore  - like the matrix ones - mounted on the floor of the upper deck, between the 2nd and 3rd side window.

- Technical Specifications -

Length: 11.490 mm
Width: 2500 mm
Height: 4060 mm

Engine: MAN D2566MUH, 141 kW at 2100 RPM
Gearbox: Voith D851
Maximum speed: 75 km/h

Empty weight: 10700 kg
Gross weight: 16.000 kg

Seats upper deck: 47
Seats lower deck: 34
Standing places: 8
[end]

